GoSurfaceMaker

Gocator高度图片生成工具

DLL: GoSurfaceMaker.dll

依赖项：kApi.dll；GoSdk.dll；commonLib.dll

程序：

'连接系统

Public Function connect(ByRef errMsg As String) As Boolean

'断开系统

Public Function disconnect(ByRef errMsg As String) As Boolean

'打开激光，开始接受轮廓线

Public Function start(Optional ByRef errMsg As String = "") As Boolean

'关闭激光

Public Function close(Optional ByRef errMsg As String = "") As Boolean

'设置编码器触发间隔

Public Function setEncoderSpacing(ByRef space As Double) As Boolean

'生成Halcon图片

Public Function getHalconImage(ByRef image As HObject) As Boolean

流程：

启动系统时：connect

关闭系统时：disconnect

扫描时：运动到点位1 –> start -> setEncoderSpacing(0.01) -> 运动到点位2 -> setEncoderSpacing(0.5) –> 运动到点位3 -> setEncoderSpacing(0.01) -> 运动到点位4 –> close -> getHalconImage